- Some pipe-related commands:
  `PIPE <FUNC>`
    Manages pipes...

    `PIPE ON` | Starts a pipe section.
    `PIPE OFF` | Ends a pipe section.
    `PIPE STOP` | Stops a running pipe section. (Covered in the section on Graphics.)

  `PANEL`
    Adds a graphical panel to the pipe.
    Closing the PANEL by clicking the 'X' in the upper corner will stop the macro.
    (Covered in detail in the section on Graphics.)
  `NOOP <IN> <OUT>`
    The `NOOP` command was created to do a No-Operation copy of data from a file to a pipe or from a pipe to a file.
    Over the years many features have been added to `NOOP` to allow it to reformat the data and perform rate-control.
  `GCONTROL PIPEMON ,, <PIPENAME>`
    Simple graphical status display for a pipe.
    One of the Debug options for a macro.
  `STATUS <FILE>`
    Can be used to view the status of a pipe.

        DataFile (BLUE)    :  ram:_wave
        Data Rep (H/D)     :  EEEI / EEEI
        Number of Elements :  1.0E9
        File Type          :  1000
        Data Format        :  CF - Complex Float
        Write Protect      :  false
        Abscissa units     :  Time (sec)
        Abscissa start     :  0.0
        Abscissa delta     :  1.0E-5
        IntHeader KeySize  :  15 bytes
        Pipe Size          :  32768 bytes
        Pipe inByte/outByte:  5.5148544E7 / 5.5115776E7
          outByte/Inlet    :  5.5115776E7 / WAVEFORM
          outByte/Outlet 1 :  5.5148544E7 / FFT
          outByte/Outlet 2 :  5.5148544E7 / DEMOD
          outByte/Outlet 3 :  5.5148544E7 / STATUS
          outByte/Outlet 4 :  <not attached>
          outByte/Outlet 5 :  <not attached>
          outByte/Outlet 6 :  <not attached>
          outByte/Outlet 7 :  <not attached>
          outByte/Outlet 8 :  <not attached>