Current Page: NeXtMidas Training X-Midas Interoperability NeXtOpt Messages Unconfigured Messages
- - - | Sending unconfigured messages to NeXtMidas: Any command started from within X-Midas with a numeric ID will automatically receive any X-Midas messages sent to it. The syntax used is the same as that used in XBC (see XBC Unconfigured Messages). The corresponding NeXtMidas message will look like this:
      NAME | X-Midas message name.
      INFO | X-Midas message info.
      DATA | `{VAL1=<val1>,VAL2=<val>,...}`
- - - Sending unconfigured messages to X-Midas: When sending a message to X-Midas, use `XM.<xmid>` as the destination ID (where `xmid` is the numeric X-Midas ID). From a macro:
          message send ID="XM.<xmid>" NAME="<name>" INFO=<info> DATA=<data>
Where `<data>` matches the structure of an unconfigured message (see XBC Unconfigured Messages).