Current Page: NeXtMidas User's Guide X-Midas Interoperability Remote Midas InterFace Diagrams
| ### RMIF Diagrams #### OPEN An `OPEN` message opens a connection to the server. The server will respond to the `OPEN` message with an `OPENED` message. #### ADDC An `ADDC` will add a connection to a pipe when given the name of the remote pipe. An `ADDC` will add a connection to an `ACK` when given `Q:ACK`. #### ACK In response to a change in the server-side macro an `ACK` can be sent to a given client. If an `ACK` is sent from the server-side macro with `null` as the remote connection, RMIF will broadcast the `ACK` to all connected clients that are listening for the `ACK`. (This is the most common form of `ACK`.) #### SET When a client sends a `SET` to the server, the `SET` is passed to the server-side macro. The server-side macro performs any necessary validity checks (bounds checks, etc.) and, if the value is modified, it responds by broadcasting the change with an `ACK` message.