    X-Midas                NeXtMidas       Function
    --------------         ----------      --------------------------------------------------------------------
    ABScissa-I             HEADERMOD       Modify abscissa fields in file header
    ACQmod-M               N/A             Enter data acquisition information into header
    ADD-H                  FCALC           Add corresponding elements of two input files
    AMFSYnc-H              N/A             Perform bit synchronization on the output of AMFDIFF ...
    ARCHive-M              ARCHIVE         Send all textual screen output to specified file or device
    ASK-I                  ASK             Prompt for keyboard entry of a results parameter value
    ATTach-I               HEADERMOD-TBD   Attach a detached header back to the file data
    AUDIOCD-H              N/A             Control a CDROM device with an audio CD
    AUXiliary-I            AUX             Set auxiliary disk/path assignments for data files
    BEEp-I                 BEEP            Emit an audio beep
    BIEXPSVI-H             SVI - TBD       Smooth with a bi-exponential window with user-specified width
    BITMask-I              N/A             Create/edit/test bit masks
    BLOckavg-H             SVI - TBD       Average blocks of file data
    BOOlean-H              FCALC           Perform boolean operation on 1 or 2 bit streams
    BREAK-I                BREAK           Exit nearest enclosing WHILE, DO or FOREACH loop
    BROwse-M               HELP/GUI        Interactive utility for browsing through command capabilities
    CALCulator-I           CALC            Implement a reverse polish pocket calculator
    CALL-I                 CALL            Invoke a macro PROCEDURE or SUBROUTINE
    CATEGory-H             N/A             Display commands according to category
    CHECkout-M             CHECKOUT        Copy necessary files of command from one option area to another
    CIRccorl-H             DSP - TBD       Circular correlates one/two input signals
    CLKCMD-H               HW - TBD        Send commands to the STL3116 via ethernet
    CNTlthin-H             THIN - TBD      Thins a data file based on values in a control file
    COMMent-I              HEADERMOD       Add/Modify comment fields in file header
    COMPAre-M              COMPARE,IF      Compare two data files
    CONCatenate-I          SEDIT - TBD     Concatenate value of string to form new results value.
    CONFigure-H            CONFIGURE       Perform configuration functions
    CONJugate-H            FCALC - CONJ    Produce complex conjugates of Type 1000 or 2000 data
    CONStant-HD            WAVEFORM        Create a Type 1000 data file with constant values
    CONTinue-I             CONTINUE        Continue iterating nearest enclosing WHILE, DO or FOREACH loop
    CONTOUR-H              N/A             Perform various contouring functions on Midas files
    CONTROL-I              GCONTROL        Macro interface for creating control panel entries
    CONVErt-H              CONVERT         Convert a Midas file data and/or header to other formats
    CONVOlve-H             DSP - TBD       Convolve input file with impulse response
    COPYHeader-H           HEADERMOD-TBD   Copy header information from reference file to output file
    CORrelate-M            DSP - TBD       Perform time domain auto-correlation or cross-correlation
    CRAyif-M               N/A             control the client side of the Cray interface
    DARray-H               FCALC - DIV     Divide each element of a file into a constant
    DATAImport-M           IMPORT/F        Put Midas header on a non-Midas data file
    DATAlist-H             DATALIST        List data elements of a Midas or text file
    DATEs-H                TIMEX           Perform various date/time transfer and conversion functions
    DBLog-M                FCALC,FFT       Convert data to dB
    DCLMap-M               N/A             Map DCLMIDAS commands to XMIDAS commands
    DCLMconv-H             N/A             Convert DCL Midas macro to X-Midas
    DEBug-I                DEBUG           Turn ON/OFF the debug modes
    DECAtenate-I           SEDIT - TBD     Remove value form string to form new ASCII result value (you can also use Java String Class directly)
    DEFaults-I             DEFAULTS        Show command defaults
    DEMOS-M                DEMO            Software demonstration macro
    DEMux-HD               FCALC           Decompose complex file into separate real and imaginary output files
    DETAch-I               FILE DETACH     Detach header from file data, or set default detach mode
    DETEct-HD              DEMOD           Detect input into AM, FM, and PM
    DIGTC-H                TBD             Extract digital time code from SMS/SDN data
    DIVide-H               FCALC           Divide file 1 by corresponding elements of file 2
    DPCo-H                 DPCO;DSP        Double precision Phase/frequency/chirp-Controlled Oscillator
    DR300_TTUNER-M         N/A             Graphical Tera Tuner controller for the DR-30X
    DSM-I                  N/A             DataStream Manager (Controls the Data Stream Managers)
    DSMCLIENT-H            N/A             Fire off a datastream manager in local mode
    DSMOdule-M             N/A             Define or show a DataStream Module for a statically linked engine
    DT202_TTUNER-M         N/A             Graphical Tera Tuner controller for the DT-202
    DT300_TTUNER-M         N/A             Graphical Tera Tuner controller for the DT-30x
    DT700_TTUNER-M         N/A             Graphical Tera Tuner controller for the DT-70x
    DUAl5000-H             DUAL5000;UCL    Compute measurements between two Type 5000 files
    DYNzoom-M              N/A             Dynamic zoom utility
    EDITList-M             GCONTROL        Generic editor for choosing multiple items from a list
    ELSE-I                 ELSE            Start macro block to be executed when IF/ELSEIF conditions fail
    ELSEIF-I               ELSEIF          Start macro block to be executed when prior IF conditions fail
    ENDIF-I                ENDIF           End an IF block
    ENDLoop-I              ENDDO           End a DO block
    ENDMode-I              N/A             Terminate the current macro
    ENDSuspend-I           TBD             Terminate all macros and return to the X-Midas prompt
    ENDWhile-I             ENDWHILE        End a WHILE block
    ENVElope-M             DSP - TBD       Detect the envelope of a pre-D signal
    ENVironment-I          ENVIRONMENT     Perform various functions on the current X-Midas/NeXtMidas environment
    ERASE-I                ERASE           Delete files
    ERROr-I                ERROR           Output an error message and terminate macro
    EXIt-I                 EXIT            Return to the operating system
    EXPLain-I              EXPLAIN         Explains a command's function, arguments, and parameter requirements
    EXPORt-I               EXPORT - TBD    Exports results parameter to operating system environment
    F3000-H                HEADERMOD       Create Type 3000 file structure (XM4+)
    FANIn-HD               FANIN;XBC       Collate records from multiple input files to a single output file
    FANOut-HD              FANOUT;XBC      Decommutate records from an input file to multiple output files
    FASTCorl-H             FASTCORrelate;DSP     Execute overlap-save FFT block cross-correlation
    FASTFilter-HD          FDFILTER;DSP    Use FFT convolution algorithm to filter data
    FCALCulator-HD         FCALC           Implement a reverse polish calculator on a vector
    FCReate-H              HEADER/CREATE   Create a header and allocate space for data file
    FFT-H                  FFT             Compute the Fast Fourier Transform of an input file
    FILEList-I             FILES           List of Midas files on Midas auxiliaries (long list of user's files in X-Midas)
    FILes-I                FILES           List of Midas files on Midas auxiliaries (short list of user's files in X-Midas)
    FILETRansp-H           TBD             Transpose rows and columns of Type 1000 or 2000 file
    FILT3000-H             TBD             Extracts records from a file based on qualifiers (XM4+)
    FINd-I                 FIND            Find file and return its full path name or URL
    FIRHlbrt-H             DSP - TBD       Create a Hilbert transform impulse response
    FIRParks-H             DSP - TBD       Design linear phase FIR filter using Parks-McClellan algorithm
    FIRWind-H              FIRWIND;DSP     Design a FIR filter using the window method
    FNAme-I                FNAME           Form a full filename from its components
    FORall-M               FORALL,FOREACH  Perform a named command on list of items or for range of numbers
    FSKSIm-H               DSP - TBD       Generate a binary FSK modulated output file with phase continuity
    FSTatistics-HD         STATISTICS      Determine file statistics
    FSVa-H                 SVI - TBD       Implement a Frame Synchronous Video Averager (Integrator)
    FSVi-HD                SVI - TBD       Implement a Frame Synchronous Video Integrator
    GATe-H                 PRI - TBD       Gate input data and store results in output file
    GENEXplain-M           GENERATE,EXP    Generate an explain file for macros, host and datastream commands
    GENmsginc-H            N/A             Generate include files for primitives that do message passing
    GETDISPlayinfo-M       N/A             Return X-Windows display information
    GETvalue-H             In-Line FILE    Extract a single results parameter from a Midas file.
    GO-I                   SYS - TBD       Continue macro execution from Suspend mode
    GOTO-I                 GOTO            Transfer macro program control to a specified label
    GROup-H                GROUP           Combine two or more inputs into a Type 3000 file
    HARDLimit-H            FCALC CLIP      Clip the input data between given limits
    HEAdermod-I            HEADERMOD       Modify/Create a Midas file header
    HELp-H                 HELP            Display online help information
    HILbert-M              DSP - TBD       Generate Hilbert transform of data file
    HISTOGram-H            HISTOGRAM       Compute the histogram of input data
    HIStory-H              HISTORY         Show the history of commands executed in the shell
    HOMEpath-I             HOMEPATH        Set user home directory
    HOMOgenize-H           RESAMPLE - TBD  Interpolate Type 3000 data to uniformly-sampled Type 1000 data
    HPStep-H               N/A             Send single command or periodically step a GPIB device via serial line
    HSHFTdec-H             TUNER;DSP       Hilbert, frequency shift, and decimate
    HW-M                   HW;HWC          Utility for controlling Hardware devices
    HWConfig-H             TBD             Configuration utility for HW Control software
    HWDriver-D             TBD             Driver for controlling Hardware devices
    IF-I                   IF              Implement a logical block if-then-else function in a macro
    IMFFT-H                IFFT - TBD      Perform multiple inverse FFTs
    IMPort-I               IMPORT - TBD    Import results parameter from operating system environment
    INFO-I                 INFO            Cause a macro to issue an informational message
    INTERLeave-M           N/A             Interleave two files into a single file
    INTERPolate-H          INTERPOLATE-TBD Interpolate data into a uniformly sampled file
    INVfft-H               IFFT - TBD      Compute the inverse FFT of an input file
    JUMP-I                 CALL            Invoke a macro PROCEDURE or SUBROUTINE
    KEYword-I              KEYWORD         Facility for displaying and changing keyword fields in a file header
    LABEL-I                LABEL           Reference point for GOTO command in a macro
    LIMit-H                LIMIT - TBD     Clip or threshold data
    LISsajous-M            N/A             Generate pretty plots from Lissajous functions
    LOADConstants-H        TBD             Load the constants into a results table
    LOCation-H             TBD             Create a single entry Type 5000 file with a Geodetic frame of reference
    LOGArithm-H            FCALC           Take logarithm of each element in data file
    LOOP-I                 DO              Implement a DO loop within a macro
                           LOOP
    LRS-H                  WAVEFORM        Create a linear recursive sequence
    MAGnitude-H            FCALC           Get magnitude of a complex or real file
    MAPMAN-H               N/A             Map manipulator for Midas maps
    MARray-HD              FCALC           Multiply each element of file by a constant.
    MASK-HF                N/A             Correlate an input signal against a set of masks
    MASter-H               N/A             Set up an X-Midas session as a controller
    MAXMin-H               MAXMIN          Find the maximum and minimum values in a data file (See also: STATISTICS)
    MEDIAnfilt-H           DSP - TBD       Median filters a data file
    MEDIT-M                EDIT            Open a command's source file for editing
    MENu-H                 MENU            List available commands
    MERGefile-H            MERGEFILE       Merge an input file to the end of an output file (Use APPEND qualifier)
                           NOOP
    MESsage-I              MESSAGE         Send or get a message to/from a message queue
    MFFT-HD                FFT             Perform multiple FFTs with overlap, windowing, and single cell output
    MFIle-I                FILE            Interface to M$FILE text file processor
    MLIst-H                MACRO           List macro
    MODUlo-H               FCALC           Perform the MODULO function on a data file
    MORPH-H                DSP - TBD       Perform a Morphological operation on a file
    MPOly-H                POLYFIT         Evaluate polynomial fit on data in a piecewise manner
    MSGmask-I              N/A             Create/edit/test masks specifying info primitive should pass
    MTRANslate-H           N/A             Translates a macro for execution
    MULT2000-H             FCALC           Multiply the values in a Type class 2000 file
    MULtiply-HD            FCALC           Multiply corresponding elements of two input files
    MUX-HD                 FCALC           Combine separate real and imaginary files into one complex file
                           MUX
    NEWRate-H              NEWRate;XBC     Synchronously or asynchronously resample an input file
    NOOP-HD                NOOP            Copy an input to an output (file, socket, HTTP, UDP)
    NORmalize-HD           NORmalize;DSP   Normalize an input file by frames
    OS-ID                  OS              Send an operating system command to the appropriate OS
    PARray-HD              FCALC           Add a constant to each element of file.
    PARse-I                PARSE           Parse a command and return components in results parameters
    PASsfilt-M             FIRWIND         Create a bandpass filter
    PAUSE-I                PAUSE           Pause for specified time or force macro into Suspend mode
    PEAKPick-H             PEAKPICK        Find one or more peaks in data
    PHAse-H                FCALC           Get phase of a complex file
    PIPE-H                 PIPE            Change the macro piping mode
    POLAr-H                FCALC           Converts rectangular to polar, with phase in degrees
    POLLtc-H               HW - TBD        Poll time code reader or CPU time
    POLYEval-H             POLYEVAL        Evaluate a polynomial using previously stored coefficients
    POLYFit-H              POLYFIT         Fit a polynomial to data
    POLYPHase-H            DSP - TBD       Emulate TMIC input filters, but with symmetric coefficients
    PRIFunc-H              PRI - TBD       Cyclically alter an X-Midas file or pipe
    PRIthin-H              PRI - TBD       Cyclically thin input data and store results in output file
    PROtect-I              FILE PROTECT    Protect files from overwriting
    PULse-M                WAVEFORM        Create a pulse of specified width and position
    QSOrt-H                SORT            Sort Type 1000, 2000, 3000, and 5000 files
    RAMp-H                 RAMP,WAVEFORM   Create a ramp (sawtooth) file
    RANDom-H               CALC            Generate a random number
    READID-I               N/A             Set X-Midas read path identification string
    RECall-I               !               Recall previously-entered command
    REFormat-H             NOOP            Change the data format of an existing file (With FT qualifier)
    RELease-M              TBD             List the current X-Midas release notes
    REMove-I               REMOVE          Remove one or more results parameters from results table
    RESET-I                TBD             Reset the environment after pipe or macro hose up
    RESults-I              RESULTS         Create and display results parameters (See Also: SET,GET)
    RETURN-I               RETURN          Return from a macro, procedure, subroutine, or control section
    RMIf-H                 RMIF            Remote Midas InterFace to communicate with remote processors
    RQFshift-HD            N/A             Real Quick Freq. SHIFT; optional filter, block avg and reformat
    RSM-IH                 N/A             Remote Session Manager (controls the Remote Sessions)
    RTLiss-M               N/A             Generate real-time Lissajous plots
    SAM-M                  N/A             Utility for controlling SnapShot Memory and its Patch Panels
    SAMDriver-H            N/A             Primitive driver for the SAM macro
    SARray-H               FCALC           Subtract each element of a file from a constant.
    SAVe-I                 FILE            Save .TMP file as .PRM (or other specified name and extension)
    SAY-I                  SAY             Echo a text line to the terminal
    SBTuner-H              TUNER;DSP       Subband tuner: input -> filter, decimate, tune -> output
    SD350-M                SD360           Software emulation of a spectral dynamic display
    SEDIT-I                SEDIT           Edit a string and write it to a results parameter
    SETNode-M              N/A             Determine plot node for X-Windows display
    SETSeed-H              WAVEFORM/SEED   Set the random number generator seed to a new value
    SINcosine-HD           WAVEFORM        Create sinusoidal data files
    SINKFile-HD            TBD             Interactively output data from a Midas file/pipe to a FILE
    SINKMBX-H              N/A             Write a Midas file/pipe to a VMS mailbox
    SINKMSG-H              RMIF,TBD        Transfer message to readers in a given range over a socket
    SINKSAM-H              N/A             Synchronize a SAM playback from a Midas file/pipe
    SINKSB-H               N/A             Write data from Midas file/pipe to SoundBlaster compatible card
    SINKSOCKet-H           NOOP            Write to a socket from a Midas file/pipe (NOOP STP://... [FILENAME])
    SKIP-I                 SKIP - TBD      Move past macro commands without executing them
    SLAve-H                N/A             Field commands from a MASTER primitive and have them executed
    SMOoth-M               FILTER          Smooth data file using rectangular filter
    SOCKETMsg-H            RMIF            Connect the message queues of two X-Midas sessions
    SOUnder-M              N/A             Run a SOUNDBLASTER spectrum analyzer/mixer/AudioCD controller
    SOURCEFile-HD          SOURCEFILE      Interactively input data from a FILE to a Midas file/pipe
    SOURCEMBX-H            N/A             Read VMS mailbox data into a Midas file/pipe
    SOURCEMSG-H            RMIF - TBD      Read messages off a socket and post them to a message queue
    SOURCESAM-HD           N/A             Synchronize a SAM acquisition into a Midas file/pipe
    SOURCESB-H             N/A             Read data from SoundBlaster compatible card into Midas file/pipe
    SOURCESOCKet-H         NOOP            Read from a socket to a Midas file/pipe (NOOP [FILENAME] STP://...)
    SPEctra-H              FFT             Perform spectral analysis of two input channels
    SPLice-H               TBD             Extract/insert subrecords/components from/to Type 3000/5000 files
    SPLit-H                SPLIT           Split a Type 3000 file into Type 1000 files
    STATEVector-H          TBD             Grab a set of state vectors from name source & convert to Type 5000 files
    STATIstics-H           STATISTICS      Determine statistics of data file
    STatus-I               STATUS          Display file header information
    STEP-I                 TBD             Execute next macro statement and return to Suspend mode
    STL3116_set-M          N/A             Basic MSL setup macro for the STL3116 clock generator
    SUBtract-H             FCALC           Subtract file 2 from file 1
    SURFDEMO-M             N/A             Macro to demonstrate use of XRTSURFace
    SVICmd-H               N/A             Send commands to STL SVI
    SWItch-I               SWITCH          Define static switches or get a switch value into a results parameter
    SYNCPlot-M             N/A             Convert sync file and plot output (AMFSYNC)
    SYntax-I               SYNTAX          Show command line syntax for the named command
    TCcmd-H                N/A             Send command to Metalize time code reader
    THIn-H                 THIN            Copy portions of one file to another
    TIMECode-I             HEADER,TIMEX    Set and retrieve time code
    TIMer-I                TIMER           Implement primitive execution and elapsed time functions
    TIMex-I                TIMEX           Implement time transfer and conversion functions
    TRACk-H                N/A             Create Type 5000 position and/or velocity files from NORAD input
    TRANSFFT-H             N/A             Perform a corner turning operation on a 2-D complex table
    TRANSform-H            TBD             Transform data between different reference frames,coordinate systems, scalings
    TRANSPose-H            TBD             Perform column/row translation
    TRAP-I                 TRAP            Branch on errors or warnings
    TTcmd-H                N/A             Send commands to Tera Tuner
    TTUNER-M               N/A             Graphical Tera Tuner controller
    TUTor-MH               TBD             User's Guide/Primitive Programmer's Guide tutorial
    TWOdthin-H             THIN            Extract rectangulare subset of 2-D (Type 2000) data file
    TYPEOF-I               IF              Get type and other information of a specified result parameter
    UBIquitous-H           FFT/PSD         Create frequency vs time spectral output for two channels
    UNGroup-H              SPLIT - TBD     Split subrecords from Type 3000/5000/6000 files into separate files
    UNIForm-H              WAVEFORM-TBD    Create file of uncorrelated uniformly distributed random numbers
    UNITs-H                N/A             List numeric codes for header units and component type names
    UNIVerse-H             N/A             Display mathematical and geophysical constants
    UNPRotect-I            FILE UNPROTECT  Remove file overwrite protections
    UNWrap-H               FCALC           Unwraps/wraps data with optional differencing
    UPDate-H               UPDATE          Update the command.cnf file for a specified option tree
    UPSample-H             RESAMPLE-TBD    Upsample a real input file by given upsampling factor
    UPZero-H               THIN            Upsample a file by inserting zeros
    USERid-I               N/A             Set user identification
    VALue-I                RES,GET         Display results parameters
    VERify-I               VERIFY          Turn ON/OFF the verify modes; echo fully-parsed commands to terminal
    WARNing-I              WARNING         Cause a macro to issue a warning message
    WAVeform-HD            WAVEFORM        Create signal waveforms of various shapes
    WHILE-I                WHILE           Implement a logical do-while loop function in a macro
    WHItenoise-H           WAVEFORM        Create an array of Gaussian white noise random values
    WIDGET-I               GCONTROL        Create a stand alone widget (/SHOW=NP All public vars can be WIDGETS)
    WINdow-H               WINDOW          Create a specified window for FFT-based functions
    WRAp-M                 FCALC           Wrap data so it lies within specified range
    WRITEID-I              N/A             Set Midas write path identification string
    XATMplot-H             PLOT - ???      Asynchronous Time, Message plotter
    XAUdiocd-M             N/A             X-windows interface to an audio CD changer
    XBHOST-O               BLD,BUILD       Low level OS utility that builds and likes HOST primitives
    XBLIB-O                BLD,BUILD       Build the library and intrinsics
    XCAll-IH               GCONTROL        An interface to most X-Midas graphical widgets
    XCFGedit-H             N/A             XWindow-based configuration parameter editor
    XCNTRL-H               GCONTROL        Primitive for running control section driven macro
    XCOlormap-H            TBD             Interactive colormap routine for X-Windows environment.
    XCONtrol-I             GCONTROL        Recognizer verb in macro controls section for creating control panel
    XDATAlist-H            LIST            X-Windows based file viewer/editor/monitor
                           LIST2
    XENVironment-M         TBD             Macro to adjust X-Windows environment settings
    XFPP-O                 BUILD           XMidas Fortran PreProcessor
                           BUILDOPT;XBC    See X-Midas Backwards Compatibility section
    XGEO-M                 GEOGUI          Demonstration macro of geographical plotting capability
    XGEOEvent-M            LAYERGEO-TBD    Dialog box to modify XGEOPLOT event records
    XGEOPlot-H             PLOT            Generate plotter for Midas files
    XMBACKUP-O             NM MAKE ZIP     Create an archive file of an option tree. (Must be run in OS shell)
    XMBld-M                BLD,BUILD       Build a command or library
    XMBOPT-M               BLD,BUILDOPT    Compile an option tree and build its support files
    XMCheckproc-H          N/A             Check if X-Midas process is running
    XMDir-O                NMD             Change or display the current working directory as X-Midas sees it
    XMKill-H               REGISTRY        Kill an X-Midas Process
    XMListprocs-H          REGISTRY,ENV    Display a list of current X-Midas processes
    XMESsage-H             TBD             A message queue monitor for X-Windows terminals
    XMOpt-O                OPTION          Display or define an option tree path
    XMPath-M               PATH            Configure command dictionary according to an option search list
    XMProclist-H           REG - TBD       Create a Type 3000 file with a list of current processes
    XMRemotes-M            N/A             Convert the REMOTES.CFG database into OS specific procedures
    XMSglog-H              MESSAGELOG      Create a window in which text messages are displayed
    XMVer-M                VERSION         Display current version of Midas or a Midas option tree
    XP3d-H                 PLOT            Generic 3D plotter for special X-Midas files
    XPANEL-H               PANEL           Draw a bare window with facilities for overlaying other windows
    XPC-O                  BLD,BUILD       X-Midas preprocess and compile utility
    XPIPE-H                PIPE,PANEL      Primitive for running a piped macro with graphical feedback
    XPLot-H                PLOT            General-purpose plotter for line plots of static data
    XRaster-H              PLOT            General-purpose raster for falling raster display of static framed data
    XRTDisplay-HD0         GCONTROL,TEXTDISPLAY  Real time results parameter display for X-windows terminal
    XRTPlot-HD0            PLOT            Realtime plotter, continually updating line plot of file or pipe data
    XRTRaster-HD0          PLOT            Realtime raster, continually updating falling raster of file or pipe data
    XRTSAMview-H           N/A             Graphical representation of SAM usage by XMidas files
    XRTSURFace-H           PLOT            Plot Type 2000 data in a surface plot orientation
    XSCAPE-M               HELP/BUILD      Browser interface
    XSEarch-M              N/A             Demo macro patterned after a signal search algorithm
    XTEXT-H                TEXTDISPLAY     Display lines of text (single font and color)
    XTUtor-M               TUTOR - TBD     Graphical tutorial on X-widgets and displays
    XVIew-H                HELP/GUI        Graphical interface to HELP, EXPLAIN, and BROWSE
    XWIndow-I              TBD             Set the X-Windows default screen, window size, and placement
    ZPIPE-H                ZPIPE;UCL       Transfer XMIDAS pipes between computers (sockets)