Current Page: NeXtMidas Training Option Trees Lab 1 Solution
- - | Lab 1 (solution): Here is what you should have done to add the option trees:
        nM> option
        Available Option Trees (<n> = index on path):
               AUDIO        = /home/burdell/nxm371/nxm/audio/
               DATABASE     = /home/burdell/nxm371/nxm/database/
           <1> DSP          = /home/burdell/nxm371/nxm/dsp/
           <2> HWC          = /home/burdell/nxm371/nxm/hwc/
               SERVLET      = /home/burdell/nxm371/nxm/servlet/
           <3> SYS          = /home/burdell/nxm371/nxm/sys/
               UCL          = /home/burdell/nxm371/nxm/ucl/
               XBC          = /home/burdell/nxm371/nxm/xbc/
        nM> path add ucl
        <Download the SAMPLEOPT option tree and expand it.>
        <In this example it was put in /home/burdell/sampleopt123.>
        nM> option sampleopt /home/burdell/sampleopt123/nxm/sampleopt
        nM> path add sampleopt
        nM> opt
        Available Option Trees (<n> = index on path):
               AUDIO        = /home/burdell/nxm371/nxm/audio/
               DATABASE     = /home/burdell/nxm371/nxm/database/
           <3> DSP          = /home/burdell/nxm371/nxm/dsp/
           <4> HWC          = /home/burdell/nxm371/nxm/hwc/
           <1> SAMPLEOPT    = /home/burdell/sampleopt123/nxm/sampleopt/
               SERVLET      = /home/burdell/nxm371/nxm/servlet/
           <5> SYS          = /home/burdell/nxm371/nxm/sys/
           <2> UCL          = /home/burdell/nxm371/nxm/ucl/
               XBC          = /home/burdell/nxm371/nxm/xbc/
  - 1. Once you've added those option trees, please answer the following questions: What is the name of the switch for the `KAISWIND` command (in DSP) that indicates that "Output response should be complex"?
           The /CMPLX switch.
    2. When you run the `DEMO` command in the SAMPLEOPT option tree, what is plotted?
           A picture of a sunset.
    3. You now have two `DEMO` commands available (one in SAMPLEOPT, the other in SYS). Which one runs when you just type `DEMO`? Can you run the other one? If so, how?
           DEMO runs the one in SAMPLEOPT, DEMO;SYS runs the one in SYS.
    4. How do you change your homepath to be the `mcr` area of SAMPLEOPT?
           nM> home mcr sampleopt
    5. How do you change your OS's working directory to the `mcr` area of SAMPLEOPT?
           $ nmd mcr sampleopt