Current Page: NeXtMidas Training RMIF & Remoting RMIF Lab Solution
- - - | Lab 1 (solution): Here is what you should have done (after `nmstart` in both terminals): In SERVER window:
          nM> sd360/server
    - In CLIENT window:
          nM> sd360/client
  - On the server window, there should have been a PSD line and a PSD raster plot that are in-sync with each other. There should have been no plot data in the client windows on startup. After clicking the OPEN button on the client window, data should flow from the server to the client. As the mouse in moved over the client green plot trace, the server trace follows and vice-versa. From the web browser, when you clicked "EXIT" link to the right of the STATE link on the "/Controls" page, it shoul have exited your sd360 server macro. (Advanced) CLIENT window on another machine (change below remote IP address appropriately):
        nM> sd360/client/remote=10.10.194.81:9000